Efficiency of Cerenkov light detection after correcting tracking of radiating particles. Slices in Z are every 10 cm. Slices are re-normalized to the maximum of the last Z slice (140-150 cm) to check ”the walk” of angular efficiency along LGD block.